<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.7.1">
<drawing>
<board>
<plain>
<wire x1="33.02" y1="78.74" x2="86.36" y2="78.74" width="0.1524" layer="20"/>
<wire x1="86.36" y1="78.74" x2="86.36" y2="60.96" width="0.1524" layer="20"/>
<wire x1="86.36" y1="60.96" x2="33.02" y2="60.96" width="0.1524" layer="20"/>
<wire x1="33.02" y1="60.96" x2="33.02" y2="78.74" width="0.1524" layer="20"/>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AUDIO-JACK">
<description>&lt;h3&gt;3.5mm Stereo Audio Jack&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:5&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Audio-3.5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;Audio_Jack&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X01_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole - No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:1&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_01&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="E$4" library="SparkFun-Connectors" package="AUDIO-JACK" value=""/>
<element name="E$5" library="SparkFun-Connectors" package="AUDIO-JACK" value=""/>
<element name="E$6" library="SparkFun-Connectors" package="AUDIO-JACK" value=""/>
<element name="E$7" library="SparkFun-Connectors" package="1X01_NO_SILK" value=""/>
<element name="E$8" library="SparkFun-Connectors" package="1X01_NO_SILK" value=""/>
<element name="E$9" library="SparkFun-Connectors" package="1X01_NO_SILK" value=""/>
<element name="E$10" library="SparkFun-Connectors" package="1X01_NO_SILK" value=""/>
<element name="E$11" library="SparkFun-Connectors" package="1X01_NO_SILK" value=""/>
<element name="E$12" library="SparkFun-Connectors" package="1X01_NO_SILK" value=""/>
<element name="E$13" library="SparkFun-Connectors" package="1X01_NO_SILK" value=""/>
<element name="E$14" library="SparkFun-Connectors" package="1X01_NO_SILK" value=""/>
<element name="E$15" library="SparkFun-Connectors" package="1X01_NO_SILK" value=""/>
<element name="E$16" library="SparkFun-Connectors" package="1X01_NO_SILK" value=""/>
<element name="E$1" library="SparkFun-Connectors" package="1X01_NO_SILK" value=""/>
<element name="E$3" library="SparkFun-Connectors" package="1X01_NO_SILK" value=""/>
<element name="E$2" library="SparkFun-Connectors" package="1X01_NO_SILK" value=""/>
<element name="E$17" library="SparkFun-Connectors" package="1X01_NO_SILK" value=""/>
<element name="E$18" library="SparkFun-Connectors" package="1X01_NO_SILK" value=""/>
</elements>
<signals>
<signal name="S$2">
</signal>
<signal name="S$1">
</signal>
<signal name="S$3">
<contactref element="E$4" pad="TIP"/>
<contactref element="E$12" pad="1"/>
</signal>
<signal name="S$4">
<contactref element="E$4" pad="RING"/>
<contactref element="E$7" pad="1"/>
</signal>
<signal name="S$5">
<contactref element="E$5" pad="TIP"/>
<contactref element="E$8" pad="1"/>
</signal>
<signal name="S$6">
<contactref element="E$5" pad="RING"/>
<contactref element="E$9" pad="1"/>
</signal>
<signal name="S$8">
<contactref element="E$6" pad="TIP"/>
<contactref element="E$10" pad="1"/>
</signal>
<signal name="S$9">
<contactref element="E$6" pad="RING"/>
<contactref element="E$11" pad="1"/>
</signal>
<signal name="GND">
<contactref element="E$13" pad="1"/>
<contactref element="E$5" pad="SLEEVE"/>
<contactref element="E$15" pad="1"/>
<contactref element="E$16" pad="1"/>
<contactref element="E$6" pad="SLEEVE"/>
<contactref element="E$1" pad="1"/>
<contactref element="E$14" pad="1"/>
<contactref element="E$4" pad="SLEEVE"/>
<contactref element="E$3" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
