<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.7.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="0" y2="17.78" width="0.1524" layer="20"/>
<wire x1="0" y1="17.78" x2="140.97" y2="17.78" width="0.1524" layer="20"/>
<wire x1="140.97" y1="17.78" x2="140.97" y2="0" width="0.1524" layer="20"/>
<wire x1="140.97" y1="0" x2="0" y2="0" width="0.1524" layer="20"/>
</plain>
<libraries>
<library name="switches">
<packages>
<package name="DIY-PUSHBUTTON">
</package>
<package name="2POS-SWITCH">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="POT-PTH-ALPS">
<description>&lt;h3&gt;9mm Square Rotary Potentiometer - PTH&lt;/h3&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/datasheets/Components/General/Linear-Trimpot.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="connectors">
<packages>
<package name="RJ45-SHIELDED">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="E$1" library="switches" package="DIY-PUSHBUTTON" value=""/>
<element name="E$2" library="SparkFun-Resistors" package="POT-PTH-ALPS" value=""/>
<element name="E$3" library="SparkFun-Resistors" package="POT-PTH-ALPS" value=""/>
<element name="E$4" library="SparkFun-Resistors" package="POT-PTH-ALPS" value=""/>
<element name="E$5" library="switches" package="2POS-SWITCH" value=""/>
<element name="E$6" library="SparkFun-Resistors" package="POT-PTH-ALPS" value=""/>
<element name="E$7" library="switches" package="DIY-PUSHBUTTON" value=""/>
<element name="E$8" library="switches" package="DIY-PUSHBUTTON" value=""/>
<element name="E$9" library="connectors" package="RJ45-SHIELDED" value=""/>
</elements>
<signals>
<signal name="SW1">
<contactref element="E$9" pad="6"/>
<contactref element="E$1" pad="1"/>
</signal>
<signal name="SW2">
<contactref element="E$8" pad="1"/>
<contactref element="E$9" pad="4"/>
</signal>
<signal name="POT1">
<contactref element="E$9" pad="8"/>
<contactref element="E$2" pad="P$2"/>
</signal>
<signal name="POT2">
<contactref element="E$9" pad="7"/>
<contactref element="E$3" pad="P$2"/>
</signal>
<signal name="PPOT3A">
<contactref element="E$5" pad="1"/>
<contactref element="E$4" pad="P$2"/>
</signal>
<signal name="POT3B">
<contactref element="E$5" pad="3"/>
<contactref element="E$6" pad="P$2"/>
</signal>
<signal name="POT3">
<contactref element="E$9" pad="5"/>
<contactref element="E$5" pad="2"/>
</signal>
<signal name="5V">
<contactref element="E$3" pad="P$3"/>
<contactref element="E$9" pad="2"/>
<contactref element="E$2" pad="P$3"/>
<contactref element="E$4" pad="P$3"/>
<contactref element="E$6" pad="P$3"/>
</signal>
<signal name="SW3">
<contactref element="E$7" pad="1"/>
<contactref element="E$9" pad="3"/>
</signal>
<signal name="GND">
<contactref element="E$8" pad="2"/>
<contactref element="E$7" pad="2"/>
<contactref element="E$6" pad="P$1"/>
<contactref element="E$9" pad="1"/>
<contactref element="E$4" pad="P$1"/>
<contactref element="E$9" pad="SH"/>
<contactref element="E$9" pad="SH1"/>
<contactref element="E$3" pad="P$1"/>
<contactref element="E$2" pad="P$1"/>
<contactref element="E$1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
